Automatic and Resuable Metal Supports for 3D Printing

Since our experimental machine is an modification of an commercial printing platform, the algorithm use the same STL file as the mesh input. To generate the final toolpath and its G-code, the